IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "bim-house-sample.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — bim-house full geometry"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "BIM.HOUSE Sample Project" | long name "BIM.HOUSE" | phase "30sqm one-story sample"
  IFCSITE "Sample Site (Tokyo)" | latitude 35° 40′ 0″ | longitude 139° 46′ 0″ | elevation above sea level 0.
    IFCBUILDING "BIM.HOUSE Sample Building" | object type "30sqm flat-roof one-story wood" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | object type "Ground Floor" | elevation 0.
        contains 6 elements
          1 x IFCSLAB | object type "Concrete 150mm" | FLOOR | names: "GF Slab"
          4 x IFCWALLSTANDARDCASE | object type "Wood CLT 120mm + insulation" | names: "Wall N", "Wall S", "Wall E" (+1 more)
          1 x IFCDOOR | object type "Wood 900x2100" | names: "Entry Door"