IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "u-40ftu-oai2cvpi-real-listing.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — Real Listing AI Design"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "コンテナの丘 ― 北海道40ft×Uコート (プール+サウナ+屋上ラウンジ)" | long name "BIM.HOUSE" | phase "2-story ISO 40ft 海上コンテナ × 6 (白塗装) + 鉄骨補強, 168sqm proposed for 900sqm lot at 北海道川上郡弟子屈町 (丘陵地・眺望)"
  IFCSITE "北海道川上郡弟子屈町 (丘陵地・眺望)" | object type "Real listing site, 900sqm" | elevation above sea level 0.
    IFCBUILDING "コンテナの丘 ― 北海道40ft×Uコート (プール+サウナ+屋上ラウンジ) (Proposed)" | object type "2F ISO 40ft 海上コンテナ × 6 (白塗装) + 鉄骨補強 168sqm" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | elevation 0.
        contains 28 elements
          1 x IFCSITE | names: "敷地 ― 北海道の丘 約900㎡" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          6 x IFCWALL | names: "西棟 40ft ― サウナ/水風呂/寝室", "南棟 40ft ― プール基盤コンテナ", "東棟 40ft+ ― 廊下/水回り" (+3 more) | material: "Generic" | property sets: Pset_WallCommon, BaseQuantities
          4 x IFCWINDOW | names: "北棟 全面ガラス引戸 (中庭側)", "ラッププール 10.5m (温水)", "水風呂 (アイスプランジ)" (+1 more) | material: "Generic" | property sets: Pset_WindowCommon, BaseQuantities
          2 x IFCSLAB | FLOOR | names: "中庭ウッドデッキ", "可動ペルゴラ (白幕・電動)" | material: "Generic" | property sets: Pset_SlabCommon, BaseQuantities
          4 x IFCCOLUMN | COLUMN | names: "ペルゴラ支柱" | material: "Generic" | property sets: Pset_ColumnCommon, BaseQuantities
          2 x IFCSOLARDEVICE | names: "屋根太陽光" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          1 x IFCRAILING | HANDRAIL | names: "屋上ガラス手摺 (西)" | material: "Generic" | property sets: Pset_RailingCommon, BaseQuantities
          6 x IFCFURNISHINGELEMENT | names: "サンラウンジャー", "シーシャ", "バーカウンター" (+1 more) | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          1 x IFCCOVERING | FLOORING | names: "ペルシャ絨毯" | material: "Generic" | property sets: Pset_CoveringCommon, BaseQuantities
          1 x IFCSTAIR | STRAIGHT_RUN_STAIR | names: "外部階段 (地上→デッキ)" | material: "Generic" | property sets: Pset_StairCommon, BaseQuantities

Property sets
  Pset_BuildingElementCommon | properties | on 3 objects (3 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "サンラウンジャー" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 2 objects (2 IFCSOLARDEVICE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "屋根太陽光" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCSITE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "敷地 ― 北海道の丘 約900㎡" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "シーシャ" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "バーカウンター" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ダイニングテーブル" (IFCLABEL)
  BaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    Length = 2.2540 [MILLI METRE]
    NetVolume = 0.0507 [CUBIC_METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALL)
    Height = 2.8960 [MILLI METRE]
    Length = 12.0000 [MILLI METRE]
    NetSideArea = 34.7520 [SQUARE_METRE]
    NetVolume = 84.7254 [CUBIC_METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCFURNISHINGELEMENT)
    NetVolume = 0.5335 [CUBIC_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCSOLARDEVICE)
    NetVolume = 0.2688 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSITE)
    NetVolume = 54.0000 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 2.8960 [MILLI METRE]
    Length = 2.4380 [MILLI METRE]
    NetSideArea = 7.0604 [SQUARE_METRE]
    NetVolume = 84.7254 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 2.8960 [MILLI METRE]
    Length = 2.4380 [MILLI METRE]
    NetSideArea = 7.0604 [SQUARE_METRE]
    NetVolume = 101.9387 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 24.0000 [SQUARE_METRE]
    NetVolume = 3.3600 [CUBIC_METRE]
    OverallHeight = 2.4000 [MILLI METRE]
    OverallWidth = 10.0000 [MILLI METRE]
  BaseQuantities: 12 more contents on 12 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "西棟 40ft ― サウナ/水風呂/寝室" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "南棟 40ft ― プール基盤コンテナ" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "東棟 40ft+ ― 廊下/水回り" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "北棟 40ft ― バー/ダイニング" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "サウナ (セルフ・セダー)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "2F 寝室コンテナ 40ft (片持ち)" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "北棟 全面ガラス引戸 (中庭側)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ラッププール 10.5m (温水)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "水風呂 (アイスプランジ)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2F ガラスラウンジ (バー/ビリヤード)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "中庭ウッドデッキ" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "可動ペルゴラ (白幕・電動)" (IFCLABEL)
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ペルゴラ支柱" (IFCLABEL)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "屋上ガラス手摺 (西)" (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ペルシャ絨毯" (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "外部階段 (地上→デッキ)" (IFCLABEL)